|  |  |
| --- | --- |
|  |  |
| Products： | 4 pillar Block Cutting Machine uses PLC system and Human-machine interface, combined with Ultra-high precision rotary encoder to slice, uses inverter to control left-right feeding , adjusts speed according to the stone material. It uses hydraulic lifting system ,combination of Chrome-plated guide pin and wear guide bush, with small gap, wearable, beautiful structure, and Guide Sleeve with multi-layer seals,with waterproof,dustproof,anti-spill,improving the service life. Forward-backward slicing uses high-precision screw nut driving, automatic slicing, main spare parts adopt imported good-quality material; The block can be placed on the ground directly and economize the worktable and its maintenance costs; The whole machine is featured with high cutting efficiency, high slicing precision, flatness of plate after cutting, high stability, easy-operating to suit granite and marble block with high value. Model can be selected if customer requires.  |
| Model and Parameter： **possible use 400 mm length of shaft, diam shaft:100 mm,diam pillars 140 mm**  |
|  | MB-2200-4D | MB-2600-4D | MB-2800-4D |
| Max. blade diameter： | 2200mm | 2600mm | 2800mm |
| Max. processing length： | 3800mm | 3500mm | 3700mm |
| Max. processing width: | 2200mm | 2200mm | 2200mm |
| Max. processing depth: | 950mm | 1150mm | 1250mm |
| Max. lifting stroke: | 1400mm | 1400mm | 1400mm |
| Water consumption | 15m³/h | 15m³/h | 15m³/h |
| Power of main motor ： | 37kw | 45kw | 55kw |
| Total power | 50kw | 58kw | 68kw |
| Dimension(L\*W\*H): | 7500\*4500\*6800mm | 7500\*4500\*6800mm | 8000\*4500\*7000mm |
| FOB Qingdao | **32000** | **32000** | **33000** |
| Цена в Украине | **51000** | **52000** | **53000** |

Удлинение полезной части вала до 50 см+55 квт двигатель + 700 долл

Удлинение полезной части вала до 55 см+55 квт двигатель + 800 долл

|  |  |
| --- | --- |
|  |  |
| Products： | Block Cutting Machine uses PLC system and Human-machine interface, combined with Ultra-high precision rotary encoder to slice, uses inverter to control left-right feeding and adjusts the speed according to the stone material. It uses hydraulic lifting system and the forward-backward slicing uses high-precision screw nut driving, automatic slicing, main spare parts adopt imported good-quality material; The block can be placed on the ground directly and economize the worktable and its maintenance costs; The whole machine is featured with high cutting efficiency, high slicing precision, flatness of plate after cutting, high stability, easy-operating to suit granite and marble block with high value. Model can be selected if customer requires.  |
| Model and Parameter： **possible use 400 mm length of shaft, diam shaft:100 mm,diam pillars 180 mm** |
| Appellation HEAVY TYPE | MB-2600-4D | MB-2800-4D | MB-3200-4D |
| Max. blade diameter： | 2600mm | 2800mm | 3200mm |
| Max. processing length： | 3500mm | 3700mm | 3300mm |
| Max. processing width: | 2200mm | 2200mm | 2200mm |
| Max. processing depth: | 1150mm | 1250mm | 1420mm |
| Max.lifting stroke: | 1400mm | 1400mm | 1600mm |
| Water consumption | 15m³/h | 15m³/h | 15m³/h |
| Power of main motor ： | 45kw | 55kw | 75kw |
| Total power | 58kw | 68kw | 88kw |
| Dimension(L\*W\*H): | 7500\*4500\*6800mm | 7500\*4500\*7000mm | 8000\*4500\*7500mm |
| Weight | 17000kg | 17500kg | 18500kg |
| Цена в Украине | **54000** | **55000** | **56000** |

|  |  |
| --- | --- |
|  |  |
| Products： | Block Cutting Machine uses PLC system and Human-machine interface, combined with Ultra-high precision rotary encoder to slice, uses inverter to control left-right feeding and adjusts the speed according to the stone material. It uses hydraulic lifting system and the forward-backward slicing uses high-precision screw nut driving, automatic slicing, main spare parts adopt imported good-quality material; The block can be placed on the ground directly and economize the worktable and its maintenance costs; The whole machine is featured with high cutting efficiency, high slicing precision, flatness of plate after cutting, high stability, easy-operating to suit granite and marble block with high value. Model can be selected if customer requires.  |
| **Fitting blades with stair type：possible use 65 cm length of shaft.** |
|  | MB-2600-4D | MB-2800-4D | MB-3200-4D |
| Max. blade diameter： | 2200mm | 2200mm | 2200mm |
| Max. processing length： | 3500mm | 3700mm | 3500mm |
| Max. processingwidth: | 2200mm | 2200mm | 2200mm |
| Max. processing depth: | 1400mm | 1400mm | 1400mm |
| Max.lifting stroke: | 920mm | 920mm | 920mm |
| Water consumption | 15m³/h | 15m³/h | 15m³/h |
| Power of main motor ： | 90kw | 90kw | 90kw |
| Dimension(L\*W\*H): | 7500\*4500\*6800mm | 8000\*4500\*6800mm | 8000\*4500\*6800mm |
| Weight | 18000kg | 18500kg | 19000kg |
| Цена в Украине | **60200** | **61800** | **62000** |