|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Product Name：：**  Automatic slabs polishing machine | 859896989168305214 | | | | | | |
| **Accessories details** | 台湾HIWIN直线导轨 Taiwan HIWIN linear guideway | | 台湾亚德客气缸  AirTAC air cylinder from Taiwan | | 台湾亚德客电磁阀(3)  AirTAC electromagnetic valve from Taiwan | | 日本安川变频器(1)(1)  Yaskawa frequency changer from Japan |
| 交流接触器(1)  Schneider AC ontactor | | 树脂磨盘专用弹性磨头  Elastic grinding head for resin abrasive | | 电控柜  Electric cabinet | | 施耐德马达保护器  Schneider motor protector |
| 板型检测装置  Model detector | | Operation panel | | 威海通达石材P掉地面盒子那一堆  Client’s workshop | | 道强石材连续磨车间2  Client’s workshop |
| **description：** | Polishing machine adopts high quality steel, where the pneumatic parts adopt YADEK products from Taiwan to reserve a compact structure and steady performance so as to improve the processing efficiency. The machine polished the surface for polishing granite slabs. Allocation the flexibility polishing heads for granite. The whole machine is featured with high polishing efficiency ,and greatly reduced abrasive consumption.  The polishing machine uses PLC system. The intelligent control is available for operator with LCD touch screen to interact with machine .Model can be selected if customer requires. | | | | | | |
| Technical data**：** | | | | | | | |
| Model： | | PL16-1000 | | PL16-1260 | | PL18-1260 | PL20-1260 |
| Количество голов | | 16 | | 16 | | 18 | 20 |
| Veolcity of conveyor belt m/min | | 0-3.5 | | 0-3.5 | | 0-3.5 | 0-3.5 |
| Swing velocity of cross spreaderm/min | | 0-48 | | 0-48 | | 0-48 | 0-48 |
| Толщина mm | | 10-50 | | 10-50 | | 10-50 | 10-50 |
| Water consumption （m³/h） | | 15-20 | | 15-20 | | 15-20 | 15-20 |
| Max ширина сляба mm | | 1000 | | 1260 | | 1260 | 1260 |
| Main motor power （kw） | | 7.5/10 | | 7.5/10 | | 7.5/10 | 7.5/10 |
| Общая мощность (kw) | | 134 | | 134 | | 152 | 167 |
| габариты（L\*W\*H）mm | | 8100\*2900\*2400 | | 8100\*3100\*2400 | | 8700\*3100\*2400 | 9300\*3100\*2400 |
| Производительность m2/12hours | | 800-1000 | | 800-1000 | | 800-1000 | 800-1000 |
| FOB price /set USD цена в порту в Китае без погрузочнно-разгрузочных модулей | | 50500 | | 51000 | | 54500 | 55000 |
| Цена в порту в Украине USD без погрузочнно-разгрузочных модулей | | 78000 | | 79500 | | 80000 | 82000 |

NOTE:1.The price of the machine include a rotor table with motor and a rotor table with blowing,also include the air vacuum pump and the gasholder.

2.The load and unload machines are not included.Prices for the load and unload machines as below:

|  |  |  |  |
| --- | --- | --- | --- |
| **Product name：**  Single arm slab vacuum lifter |  | | |
| **description：** | As a auxiliary equipment for multi-head continuous polishing machine, automatic loading and unloading machine adopt PLC programmable to combine and control the inverter , encoder, the mechanical, pneumatic, electrical to accomplish perfect action. It will load and unload the polishing slab automatic. The lifting system adopt Stable, good orientation four bar mechanism structure. It have high degree of automation, simple structure, easy operation, space-saving, stable operation and so on advance features. The whole process without manual operation, It will save 2-3 people to operating the polishing machine and will improve production efficiency by 1.5 times for continuous polishing machine and other related equipment. | | |
| Technical data**：** | | | |
| Overall dimension（L\*W\*H）mm | | **3400\*1600\*3500** | **3400\*1600\*3700** |
| Max distance of lifting mm | | **1000** | **1200** |
| Max moving distance \mm | | **1600** | **1600** |
| Max lifting weight kg | | **500** | **500** |
| Max lifting slab size mm | | **1400\*3000\*50** | **1400\*3000\*50** |
| Всего цена в порту в Китае | | **17500USD за 2 комплекта** | **18500 за 2 комплекта** |
| Всего в порту в Украине USD | | **20800USD за 2 комплекта** | **21800 за 2 комплекта** |