a

|  |  |
| --- | --- |
| Product Name  |  |
| Products： | Bridge type single blade stone cutting machine has simple and reasonable structure, high stability.It adopts hydraulic slide plate to up and down ,which has fast lifting speed, anti abrasion,not easy to deformation,convenient maintenance and so on characters.Stone processing shall be placed on the tramcar.The machine is suitable for cutting block materials. |
| Model and Parameter：перемещение в ручную на следующий рез, автоматическое перемещие на следующий рез +800 долл |
| Appellation | DT-2000 | DT-2200 | DT-2600 |
| Max. blade diameter： | 2000mm | 2200mm | 3000mm |
| Max. processing length： | 3100/3600mm | 3600mm | 4800mm |
| Worktable size(L\*W)： | 1700\*1700mm | 1700\*1700mm | 2000\*2000mm |
| Max. lifting stroke: | 900/1100mm | 1100/1300mm | 1300mm |
| Power of main motor ： | 30kw | 37kw | 37kw |
| Total power | 35.25kw | 42.25kw | 42.25kw |
| Dimension(L\*W\*H): | 7300\*5150\*5210mm | 7800\*5150\*6000mm | 9300\*5150\*7100mm |
| Weight | ±7000kg | ±7500kg | ±8500kg |
| В Украине | 22500 долл | 23500 долл  | 27000 долл |